**Список оргтехники, имеющие отслеживающий код.**

|  |  |  |  |
| --- | --- | --- | --- |
| **Производитель** | **Модель** | **точки?** | **Комментарии** |
| Brother | | | |
|  | HL-2700CN | yes | volunteer test |
|  | HL-4200CN | yes | EFF test |
| Canon | | | |
|  | CLC 1000 | yes | EFF test |
|  | CLC 2400 | yes | EFF test |
|  | CLC 3002 | yes | EFF test |
|  | CLC 4000 | yes | EFF test |
|  | CLC 5000+ | yes | EFF test |
|  | CLC-iR 3200-C1 | yes | EFF test |
|  | Color imageRUNNER C2570 | yes | EFF test |
|  | Color imageRUNNER C3100CN | yes | EFF test |
|  | Color imageRUNNER C3200 | yes | EFF test |
|  | Color imageRUNNER C3200N | yes | EFF test |
|  | Color imageRUNNER C3220 | yes | EFF test |
|  | Color Laser Copier 1150 | yes | EFF test |
|  | Imageclass MF8170C | yes | EFF test |
|  | LBP 2410 | unclear | faint dots; could be artifacts |
| Dell | | | |
|  | 3000CN | yes | EFF test |
|  | 3100CN | yes | EFF test |
|  | 5100CN | yes | EFF test |
| Epson | | | |
|  | AcuLaser C900 | yes | EFF test |
|  | AcuLaser C1100 | yes | EFF test |
|  | AcuLaser C1500 | yes | EFF test |
|  | AcuLaser C1900 | yes | EFF test |
|  | AcuLaser C3000 | yes | EFF test |
|  | AcuLaser C4000 | yes | EFF test |
| *Fuji: see [Xerox](https://www.eff.org/pages/list-printers-which-do-or-do-not-display-tracking-dots" \l "xerox)* | | | |
| Hewlett-Packard | | | |
|  | Color LaserJET 1550L | yes | EFF test |
|  | Color LaserJET 1600 | yes | EFF test |
|  | Color LaserJET 2250LN | no (??) | EFF test |
|  | Color LaserJET 2500 | yes | EFF test |
|  | Color LaserJET 2500L | yes | EFF test |
|  | Color LaserJET 2500N | yes | EFF test |
|  | Color LaserJET 2550 | yes | EFF test |
|  | Color LaserJET 2550L | yes | EFF test |
|  | Color LaserJET 2550N | yes | EFF test |
|  | Color LaserJET 2600N | yes | EFF test |
|  | Color LaserJET 2680 | yes | EFF test |
|  | Color LaserJET 2700N | yes | volunteer test |
|  | Color LaserJET 2840 | yes | EFF test |
|  | Color LaserJET 3500 | yes | EFF test |
|  | Color LaserJET 3550 | yes | EFF test |
|  | Color LaserJET 3600DN | yes | EFF test |
|  | Color LaserJET 3700 | yes | EFF test |
|  | Color LaserJET 3700DN | yes | EFF test |
|  | Color LaserJET 3700N | yes | EFF test |
|  | Color LaserJET 4500 | no | EFF test |
|  | Color LaserJET 4500DN | no | EFF test |
|  | Color LaserJET 4500N | no | EFF test |
|  | Color LaserJET 4550 | no | EFF test |
|  | Color LaserJET 4550N | no | EFF test |
|  | Color LaserJET 4600 | yes | EFF test |
|  | Color LaserJET 4600DN | yes | EFF test |
|  | Color LaserJET 4600HDN | yes | EFF test |
|  | Color LaserJET 4600N | yes | EFF test |
|  | Color LaserJET 4650 | yes | EFF test |
|  | Color LaserJET 4650DN | yes | EFF test |
|  | Color LaserJET 4650DTN | yes | EFF test |
|  | Color LaserJET 4700 | yes | volunteer test |
|  | Color LaserJET 4700DN | yes | volunteer test |
|  | Color LaserJET 4700DTN | yes | volunteer test |
|  | Color LaserJET 5M | no | EFF test |
|  | Color LaserJET 5100CN | yes | EFF test |
|  | Color LaserJET 5500 | yes | EFF test |
|  | Color LaserJET 5500ATN | yes | EFF test |
|  | Color LaserJET 5500DN | yes | EFF test |
|  | Color LaserJET 5500HDN | yes | EFF test |
|  | Color LaserJET 5550 | yes | EFF test |
|  | Color LaserJET 5550DN | yes | EFF test |
|  | Color LaserJET 5550DTN | yes | EFF test |
|  | Color LaserJET 8500 | no | EFF test |
|  | Color LaserJET 8500DN | no | EFF test |
|  | Color LaserJET 8550 | no | EFF test |
|  | Color LaserJET 8550DN | no | EFF test |
|  | Color LaserJET 8550GN | no | EFF test |
|  | Color LaserJET 9500 | yes | EFF test |
|  | Color LaserJET 9500HDN | yes | EFF test |
|  | Color LaserJET 9500MFP | yes | EFF test |
| IBM | | | |
|  | Infoprint Color 1454 | unclear | dithering? |
|  | Infoprint Color 1464 PS3 | yes | dithering? |
| Konica    (Konica/Minolta) | | | |
|  | Bizhub C252 | yes | EFF test |
|  | Bizhub C350 | yes | EFF test |
|  | Colorforce 1501 | yes | EFF test |
|  | Colorforce 8050 | yes | EFF test |
|  | DialtaColor CF 2001 | unclear | dithering? |
|  | DialtaColor CF 2002 | unclear | dithering? |
|  | Ikon CPP500E | yes | EFF test |
|  | Magicolor 2 Desklaser | no | EFF test |
|  | Magicolor 2200 DL | yes | EFF test |
|  | Magicolor 2210 | yes | EFF test |
|  | Magicolor 2300 DL | yes | EFF test |
|  | Magicolor 2300 W | yes | EFF test |
|  | Magicolor 2350 | yes | EFF test |
|  | Magicolor 2350 EN | yes | EFF test |
|  | Magicolor 2400 W | yes | EFF test |
|  | Magicolor 2430 DL | yes | EFF test |
|  | Magicolor 2450 | yes | EFF test |
|  | Magicolor 3100 | yes | EFF test |
|  | Magicolor 3300 | yes | EFF test |
|  | Magicolor 5450 | yes | EFF test |
|  | Magicolor 7300 | yes | EFF test |
| Kyocera | | | |
|  | C2630D | yes | EFF test |
|  | FS-C5016N | yes | EFF test |
|  | FS-C5020N | yes | EFF test |
|  | FS-C5030N | yes | EFF test |
|  | FS-C8008 | yes | EFF test |
|  | Mita KM-C2230 | yes | EFF test |
| Lanier | | | |
|  | LD238C | yes | EFF test |
|  | LP125CX/LP126CN | yes | EFF test |
| Lexmark | | | |
|  | C510 | yes | EFF test |
|  | C720 | unclear | retest |
|  | C752 | yes | EFF test |
|  | C752N | yes | EFF test |
|  | C760 | yes | EFF test |
|  | C910 | yes | EFF test |
|  | C912 | yes | EFF test |
| *Minolta: see [Konica](https://www.eff.org/pages/list-printers-which-do-or-do-not-display-tracking-dots" \l "konica)* | | | |
| NRG | | | |
|  | DSc38 | yes | EFF test |
| OkiDATA     (Oki) | | | |
|  | C5100 | no | EFF test |
|  | C5150 | no | EFF test |
|  | C5150N | no | EFF test |
|  | C5200 | no | EFF test |
|  | C5300 | no | EFF test |
|  | C7200 | no | EFF test |
|  | C7350 | no | EFF test |
|  | C7400 | no | EFF test |
|  | C7400N | no | EFF test |
|  | C9200 | no | EFF test |
|  | C9300 | no | EFF test |
|  | C9400 | no | EFF test |
|  | MIP C5540 | no | EFF test |
|  | OkiLAN 8100E | no | EFF test |
| Panasonic | | | |
|  | Workio KXCL-500 | yes | EFF test |
| Ricoh     *(see also [Savin](https://www.eff.org/pages/list-printers-which-do-or-do-not-display-tracking-dots" \l "savin))* | | | |
|  | Aficio 1224C | yes | EFF test |
|  | Aficio 1232C | yes | EFF test |
|  | Aficio CL 2000 | yes | press report |
|  | Aficio CL 3000 | yes | EFF test |
|  | Aficio CL 3000E | yes | EFF test |
|  | Aficio CL 6010 | yes | EFF test |
|  | Aficio CL 7000 | yes | EFF test |
|  | AP 206 | yes | EFF test |
|  | Infotec/Danka ISC 2838 | yes | EFF test |
| Samsung | | | |
|  | CLP-500 | no | EFF test |
|  | CLP-510 | no | EFF test |
|  | CLP-550 | no | EFF test |
|  | CLP-550N | no | EFF test |
| Savin | | | |
|  | C3210 | yes | EFF test |
|  | CLP35 | yes | EFF test |
| *Tektronix: see [Xerox](https://www.eff.org/pages/list-printers-which-do-or-do-not-display-tracking-dots" \l "xerox)* | | | |
| Toshiba | | | |
|  | eStudio 210c | yes | mfr. statement |
|  | eStudio 211c | yes | mfr. statement |
|  | eStudio 310c | yes | mfr. statement |
|  | eStudio 311c | yes | mfr. statement |
|  | eStudio 2100c | yes | mfr. statement |
|  | eStudio 3100c | yes | mfr. statement |
|  | eStudio 3511 | yes | EFF test |
|  | FC15 | yes | mfr. statement |
|  | FC15i | yes | mfr. statement |
|  | FC22 | yes | mfr. statement |
|  | FC22i | yes | mfr. statement |
|  | FC25P | yes | mfr. statement |
|  | FC25Pi | yes | mfr. statement |
|  | FC70 | yes | mfr. statement |
| Xerox   (Tektronix) | | | |
|  | DocuColor 12 | yes | EFF test |
|  | DocuColor 40 | yes | EFF test |
|  | DocuColor 1521 | yes | EFF test |
|  | DocuColor 1632 | yes | EFF test |
|  | DocuColor 2000 | yes | mfr. statement |
|  | DocuColor 2045 | yes | EFF test |
|  | DocuColor 2240 | yes | EFF test |
|  | DocuColor 3535 | yes | EFF test |
|  | DocuColor 5252 | yes | EFF test/mfr. statement |
|  | DocuColor 6060 | yes | EFF test/mfr. statement |
|  | Phaser 560 | no | EFF test |
|  | Phaser 740 | no | EFF test |
|  | Phaser 750 (Z750V) | no | EFF test |
|  | Phaser 750P | no | EFF test |
|  | Phaser 790 | yes | EFF test |
|  | Phaser 850DP | no | EFF test |
|  | Phaser 860DP | no | EFF test |
|  | Phaser 1235 | no | EFF test |
|  | Phaser 6100 | no | EFF test |
|  | Phaser 6200 | no | EFF test |
|  | Phaser 6200DP | no | EFF test |
|  | Phaser 6250DP | no | EFF test |
|  | Phaser 6350DP | no | EFF test |
|  | Phaser 7300DN | no | EFF test |
|  | Phaser 7300DT | no | EFF test |
|  | Phaser 7700 | no | EFF test |
|  | Phaser 7750DN | no | EFF test |
|  | Phaser 8200DP | no | EFF test |
|  | Phaser 8200DX | no | EFF test |
|  | Phaser 8400 | no | dithering? |
|  | Phaser 8400B | unclear | dithering? |
|  | Phaser 8400DP | unclear | dithering? |
|  | Phaser 8400DX | unclear | dithering? |
|  | Phaser 8400N | unclear | dithering? |
|  | Phaser 8440DP | unclear | dithering? |
|  | Phaser 8550 | no | EFF test |
|  | Phaser 8550DP | no | EFF test |
|  | Phaser 8560MFP/D | no | EFF test |
|  | WorkCentre M24 | yes | EFF test |
|  | WorkCentre Pro *(all models)* | yes | mfr. statement |

Первоисточник: <https://www.eff.org/pages/list-printers-which-do-or-do-not-display-tracking-dots>